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North Sunderland Harbour Risk Assessment FormReference: MRA 1

	Service
	North Sunderland Harbour - MRA Number 1
	Date of Risk Assessment
	07/05/2026

	Assessor
	Fiona Kibby 

	Process or Activity
	Harbour Staff General Duties



	Describe the location where activities are taking place
	
North Sunderland Harbour quays, jetties, pontoons and slipways.


	Describe the activities being undertaken
	
General care and maintenance of Harbour areas


	Describe the equipment and/ or substances being used
	
North Sunderland Harbour ladders, slipways, pontoon and quayside



	Describe the people involved in these activities (and others who might be affected)
	
Harbour staff, contractors, commercial fishermen, tripping boat crew, divers, RNLI crew, leisure users and members of the public. 



	Associated Risk Assessments
	
ALL MRAs

	Associated Safe Systems of Work
	
Port Marine Safety Code.
Guide to Good Practice. 
NSH maintenance programme.  



	Risk Rating
	Action

	20-25
	Stop Activity and Take Immediate Action

	15-20
	Urgent Action

	8-12
	Action

	3-6
	Monitor

	1 -2
	No Action – ensure controls are maintained and reviewed



	Hazard
	Uncontrolled Risk Score
	Risk Mitigations
	Residual Risk Score

	
	L
	C
	R
	
	L
	C
	R

	
Harbour staff slips or falls from height on harbour property


	
2
	
4
	
8
	
1. [bookmark: _Hlk146715162]All harbour staff are advised to self declare their fitness to work and not attend work if unable to work safely.
2. All harbour staff wear safety footwear.
3. All harbour staff wear 150N lifejackets when working on pontoon, directly above or on water.
4. [bookmark: _Hlk146715206]Guardrail and Armco barriers are surveyed 2 yearly and a regular programme of maintenance & replacement in place.      
5. [bookmark: _Hlk146715244]Harbour staff and commercial users are first aid trained. 
6. [bookmark: _Hlk146715340]Harbour lifebuoys are surveyed and inspected monthly.   
7. Harbour staff have appropriate PPE.
8. Ladders, slipways, steps and pontoon are cleaned by harbour staff regularly to avoid marine growth.
9. Ladders are surveyed 2 yearly and a regular programme of maintenance & replacement in place.
10. Maintenance that requires working from height will be carried out by 2 or more persons




	
2
	
2
	
4

	
Harbour staff is injured as a result of using hand or power tools whilst carrying out general duties
	
2
	
4
	
8
	
1. Harbour staff are provided with PPE including ear defenders, goggles, gloves and boots and will wear PPE appropriate to duties
2. All harbour staff are advised to self declare their fitness to work and not attend work if unable to work safely.
3. Harbour staff and commercial users are first aid trained.
4. Harbour staff are familiar with tools being used and will ask for assistance if required.
5. First aid kits are available to staff
6. Harbour staff are only able to carry out duties approved by the Harbour Master

	
2
	
2
	
4

	
Harbour staff is injured as a result of lifting heavy load
	
3
	
4
	
12
	
1. Harbour staff are trained in manual lifting
2. All harbour staff are advised to self declare their fitness to work and not attend work if unable to work safely
3. Harbour staff are trained in the use of the forklift and cranes and will use these in preference to manual lifting
4. Where the use of forklift or cranes is not appropriate staff will work together or request assistance when lifting heavy loads manually
5. Forklift and lifting equipment is LOLER compliant and tested regularly.

	
2
	
3
	
6

	
Harbour staff falls ill due to contact with hazardous substance such as chemicals, dust or vapour
	
2

	
4
	
8
	
1. All harbour staff are advised to self declare their fitness to work and not attend work if unable to work safely
2. Harbour staff and commercial users are first aid trained.
3. Hazardous substances will be replaced with safer products where possible.
4. Hazardous substances will be stored in a COSHH cupboard and clearly labelled.
5. PPE including gloves, face masks and eye protection is provided to staff and will be worn when appropriate to duties being carried out.
6. Regular inventory checks will be carried out by harbour staff to ensure that substances are stored correctly, not damaged and in a clean and tidy environment.
7. Substances will be used in line with the product advice guides and in ventilated spaces.
	
2
	
2
	
4
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Risk Rating Calculator
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Likelihood that hazardous event will occur Consequence of hazardous event
1 very unlikely 1 insignificant — no injury
2 unlikely 2 minor - minor injuries needing first aid
3 Tairly likely 3 moderate — up to three days’ absence
4 likely 4 major — more than seven days’ absence
5 very likely 5 catastrophic - death
Action Level Table
Risk rating Action
20-25 Stop — stop activity and take immediate action
15-16 Urgent action — take immediate action and stop activity if necessary, maintain existing controls rigorously
8-12 ‘Action — improve within specified timescale
3-6 Monitor — look to improve at next review or if there s a significant change
1-2 No action - no further action but ensure controls are maintained and reviewed

Example risk assessment

Description of hazard Who might be What risk controls | Current risk Avre further Date to be Residual risk
and hazardous event harmed? are currently in rating* controls needed? completed by rating*
lace?
i L|C R L|C R
8 rﬂhng car wntr‘\‘ petrol, Persor:wLﬁ\hng vehicle | Auto pumpAcu‘l off, 4 |2 |8 Make avawla‘ble . By next week 2 |6

[ 11038% Page30f3 | R

- ]




image2.png




