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North Sunderland Harbour Risk Assessment FormReference: MRA 5

	Service
	North Sunderland Harbour - MRA Number 5
	Date of Risk Assessment
	2 Apr 2026

	Assessor
	Fiona Kibby

	Process or Activity
	Allision



	Describe the location where activities are taking place
	
North Sunderland Harbour and approaches.


	Describe the activities being undertaken
	
Vessel makes contact with a fixed object, either port infrastructure or moored vessel.


	Describe the equipment and/ or substances being used
	



	Describe the people involved in these activities (and others who might be affected)
	
Harbour Staff, commercial fishermen, tripping boat crew, divers, RNLI crew, leisure users and members of the public. 


	Associated Risk Assessments
	
MRAs 3, 4, 6, 7, 11

	Associated Safe Systems of Work
	
North Sunderland Harbour Mooring Policy – 2023.
Colregs. 





	Risk Rating
	Action

	20-25
	Stop Activity and Take Immediate Action

	15-20
	Urgent Action

	8-12
	Action

	3-6
	Monitor

	1 -2
	No Action – ensure controls are maintained and reviewed



	Hazard
	Uncontrolled Risk Score
	Risk Mitigations
	Residual Risk Score

	
	L
	C
	R
	
	L
	C
	R

	
Vessel makes contact with a fixed object, either harbour infrastructure or moored vessel.
	
2
	
4
	
8
	
1. Vessels are crewed by suitably qualified professionals.
2. Fishing & Commercial vessels governed by MCA regulations for equipment, serviceability and crew fitness and manning levels.   
3. [bookmark: _Hlk146722654]NSH see vessel insurance, survey and crew qualifications annually.
4. NSH maintains harbour aids to navigation and quayside lighting sufficient to aid navigation.
5. Speed limit in the harbour is 3 knots – meaning any collision is likely to be low energy.  
  
	
1
	
4
	
4
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Risk Rating Calculator
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Likelihood that hazardous event will occur Consequence of hazardous event
1 very unlikely 1 insignificant — no injury
2 unlikely 2 minor - minor injuries needing first aid
3 Tairly likely 3 moderate — up to three days’ absence
4 likely 4 major — more than seven days’ absence
5 very likely 5 catastrophic - death
Action Level Table
Risk rating Action
20-25 Stop — stop activity and take immediate action
15-16 Urgent action — take immediate action and stop activity if necessary, maintain existing controls rigorously
8-12 ‘Action — improve within specified timescale
3-6 Monitor — look to improve at next review or if there s a significant change
1-2 No action - no further action but ensure controls are maintained and reviewed

Example risk assessment

Description of hazard Who might be What risk controls | Current risk Avre further Date to be Residual risk
and hazardous event harmed? are currently in rating* controls needed? completed by rating*
lace?
i L|C R L|C R
8 rﬂhng car wntr‘\‘ petrol, Persor:wLﬁ\hng vehicle | Auto pumpAcu‘l off, 4 |2 |8 Make avawla‘ble . By next week 2 |6

[ 11038% Page30f3 | R

- ]




image2.jpg




