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North Sunderland Harbour Risk Assessment FormReference: MRA 9

	Service
	North Sunderland Harbour - MRA Number 9
	Date of Risk Assessment
	2 Apr 2026

	Assessor
	Fiona Kibby

	Process or Activity
	Vehicles vs Pedestrians 



	Describe the location where activities are taking place
	
North Sunderland Harbour and approaches.


	Describe the activities being undertaken
	
Vehicles vs Pedestrians 

	Describe the equipment and/ or substances being used
	



	Describe the people involved in these activities (and others who might be affected)
	
Harbour Staff, commercial fishermen, tripping boat crew, divers, RNLI crew, leisure users and members of the public. 


	Associated Risk Assessments
	
MRAs 3, 4, 5, 6, 7, 11

	Associated Safe Systems of Work
	
North Sunderland Harbour Vessel Licensing Policy – 2023.
 




	Risk Rating
	Action

	20-25
	Stop Activity and Take Immediate Action

	15-20
	Urgent Action

	8-12
	Action

	3-6
	Monitor

	1 -2
	No Action – ensure controls are maintained and reviewed



	Hazard
	Uncontrolled Risk Score
	Risk Mitigations
	Residual Risk Score

	
	L
	C
	R
	
	L
	C
	R

	
Trailer, boat or vehicle out of control on the public slipway.
	
2
	
4
	
8
	
1. [bookmark: _Hlk147755946][bookmark: _Hlk147755916]Access to public slipway controlled by NSH staff during office hours.
2. Single launch or recovery permitted.
3. Members of public not allowed access to slipway. 
4. Slipways cleaned periodically by NSH staff.
5. Slipway gradient is very low.    
  
	
1
	
4
	
4

	
Pedestrian is hit by vehicle on NSH road / quayside.
	
4
	
4
	
16
	
1. [bookmark: _Hlk147843398]Speed limit on NSH road is 5mph.
2. Trip boat passengers are carefully marshalled by trip boat staff. 
3. Option to install speed humps remains open.
4. Option to install protected walkways remains open.
5. Option to install speed camera sign remains open.
6. Monitor number of instances / close calls.
     
	
2
	
2
	
4

	[bookmark: _Hlk147843412]
Pedestrian is hit by load being handled on NSH quayside.

	
4
	
4
	
16
	
1. Members of public not allowed on commercial quaysides where catch is landed (middle and short piers).   
2. All hoists, the forklift and cranes are LOLER compliant and tested regularly.
3. Forklift are driven by qualified personnel.
4. Crane are operated by harbour users following instructions.    
	
2
	
2
	
4

	
Pedestrian or vehicle is hit by RNLI launch trailer during emergency launch.

	
4
	
4
	
16
	
1. RNLI staff are trained in launching techniques.
2. 2 x banksmen are in attendance for each launch. 
3. NSH road is closed for launch and recovery of RNLI vessels.
4. RNLI personnel wear appropriate PPE.
5. RNLI launching does not break NSH speed limit of 5 mph.
  
	
2
	
2

	
4
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Risk Rating Calculator
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Likelihood that hazardous event will occur Consequence of hazardous event
1 very unlikely 1 insignificant — no injury
2 unlikely 2 minor - minor injuries needing first aid
3 Tairly likely 3 moderate — up to three days’ absence
4 likely 4 major — more than seven days’ absence
5 very likely 5 catastrophic - death
Action Level Table
Risk rating Action
20-25 Stop — stop activity and take immediate action
15-16 Urgent action — take immediate action and stop activity if necessary, maintain existing controls rigorously
8-12 ‘Action — improve within specified timescale
3-6 Monitor — look to improve at next review or if there s a significant change
1-2 No action - no further action but ensure controls are maintained and reviewed

Example risk assessment

Description of hazard Who might be What risk controls | Current risk Avre further Date to be Residual risk
and hazardous event harmed? are currently in rating* controls needed? completed by rating*
lace?
i L|C R L|C R
8 rﬂhng car wntr‘\‘ petrol, Persor:wLﬁ\hng vehicle | Auto pumpAcu‘l off, 4 |2 |8 Make avawla‘ble . By next week 2 |6
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